DECLARATION OF PERFORMANCE
No: PD 1304.
Unique identification code of the product-type: PA33CL50

Product: 33CL50

Intended use of the construction: Walls

Manufacturer: Isolamin Sweden AB  Industrivägen 5  95632 Överkalix Sweden

System: 3

Standard: EN 14509;2006 / AZ 2008

SP Technical Research Institute of Sweden no 1002 report 0402-CPD-P605003B

DBI Danish Institute of Fire and Security Technology no 0845 report PC 10104

Declared performance:
Essential characteristics  	Performance	Harmonised technical specification	
Tensile strength	NPD	EN 14509:2006	
Shear strength	NPD	EN 14509:2006	
Shear modulus	NPD	EN 14509:2006	
Compressive strength	NPD	EN 14509:2006	
Wrinkling stress	NPD	EN 14509:2006	
Reaction to fire	A2;s1;d0	EN 13501-1:2007 	
Fire Resistance	E 120 ; EI 20	EN 13501-2:2007+A1	
Fire Protection Ability	NPD	EN 14509:2006	
Thermal Resistance	NPD	EN 14509:2006	
Water permeability	NPD	EN 12865	
Air permeability	NPD	EN 11214	
Water vapour permeability	NPD	EN 14509:2006	
Airbone sound insulation	34 Rw	EN ISO 717-1 Rw	
Sound absorption	NPD	EN ISO 11654	
Dimentioal Variation	PASS	EN 14509:2006	
Durability	PASS	EN 14509:2006	

Technical & QA
Anders Johansson

Överkalix  2013-06-30